(export (version D)
  (design
    (source /home/jboone/src/portapack-hackrf/hardware/portapack_h1/portapack_h1.sch)
    (date "Tue 13 Jun 2017 09:42:43 PM PDT")
    (tool "Eeschema 4.0.6-e0-6349~52~ubuntu17.04.1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "PortaPack H1")
        (company "ShareBrained Technology, Inc.")
        (rev 20170522)
        (date 2017-05-22)
        (source portapack_h1.sch)
        (comment (number 1) (value "Copyright © 2014-2017 Jared Boone"))
        (comment (number 2) (value "License: GNU General Public License, version 2"))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 2) (name /audio/) (tstamps /53A8BFC3/)
      (title_block
        (title "PortaPack H1")
        (company "ShareBrained Technology, Inc.")
        (rev 20170522)
        (date 2017-05-22)
        (source audio.sch)
        (comment (number 1) (value "Copyright © 2014-2017 Jared Boone"))
        (comment (number 2) (value "License: GNU General Public License, version 2"))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 3) (name /lcd_sw_sd/) (tstamps /53A9129D/)
      (title_block
        (title "PortaPack H1")
        (company "ShareBrained Technology, Inc.")
        (rev 20170522)
        (date 2017-05-22)
        (source lcd_sw_sd.sch)
        (comment (number 1) (value "Copyright © 2014-2017 Jared Boone"))
        (comment (number 2) (value "License: GNU General Public License, version 2"))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 4) (name /hackrf_if/) (tstamps /53A8C780/)
      (title_block
        (title "PortaPack H1")
        (company "ShareBrained Technology, Inc.")
        (rev 20170522)
        (date 2017-05-22)
        (source hackrf_if.sch)
        (comment (number 1) (value "Copyright © 2014-2017 Jared Boone"))
        (comment (number 2) (value "License: GNU General Public License, version 2"))
        (comment (number 3) (value ""))
        (comment (number 4) (value ""))))
    (sheet (number 5) (name /power/) (tstamps /58CFF3E3/)
      (title_block
        (title "PortaPack H1")
        (company "ShareBrained Technology, Inc.")
        (rev 20170522)
        (date 2017-05-22)
        (source power.sch)
        (comment (number 1) (value "Copyright © 2014-2017 Jared Boone"))
        (comment (number 2) (value "License: GNU General Public License, version 2"))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref H2)
      (value HOLE1)
      (footprint hole:HOLE_3200UM_VIAS)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BBD8))
    (comp (ref H3)
      (value HOLE1)
      (footprint hole:HOLE_3200UM_VIAS)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BBEC))
    (comp (ref H4)
      (value HOLE1)
      (footprint hole:HOLE_3200UM_VIAS)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BC00))
    (comp (ref H5)
      (value HOLE1)
      (footprint hole:HOLE_3200UM_VIAS)
      (libsource (lib hole) (part HOLE1))
      (sheetpath (names /) (tstamps /))
      (tstamp 5369BC14))
    (comp (ref FID1)
      (value FIDUCIAL)
      (footprint fiducial:FIDUCIAL_65MIL)
      (libsource (lib fiducial) (part FIDUCIAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B309AC))
    (comp (ref FID2)
      (value FIDUCIAL)
      (footprint fiducial:FIDUCIAL_65MIL)
      (libsource (lib fiducial) (part FIDUCIAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B30B4C))
    (comp (ref FID3)
      (value FIDUCIAL)
      (footprint fiducial:FIDUCIAL_65MIL)
      (libsource (lib fiducial) (part FIDUCIAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B30CEC))
    (comp (ref FID4)
      (value FIDUCIAL)
      (footprint fiducial:FIDUCIAL_65MIL)
      (libsource (lib fiducial) (part FIDUCIAL))
      (sheetpath (names /) (tstamps /))
      (tstamp 53B30E8C))
    (comp (ref R11)
      (value 33R)
      (footprint ipc_resc:IPC_RESC1608X55L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0733RL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C264))
    (comp (ref R12)
      (value 33R)
      (footprint ipc_resc:IPC_RESC1608X55L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-0733RL))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C26A))
    (comp (ref C22)
      (value 220N)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM188R71A224KA01D))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C27E))
    (comp (ref C23)
      (value 220N)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM188R71A224KA01D))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C284))
    (comp (ref R18)
      (value 2K2)
      (footprint ipc_resc:IPC_RESC1608X55L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name Part) RC0603FR-072K2L))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C29C))
    (comp (ref C25)
      (value 1U)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM188R61C105KA93D))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2A2))
    (comp (ref P2)
      (value TRRS_SW_JACK)
      (footprint cui:CUI_SJ-43516-SMT)
      (datasheet http://www.cui.com/product/resource/sj-4351x-smt-series.pdf)
      (fields
        (field (name Mfr) CUI)
        (field (name Part) SJ-43514-SMT))
      (libsource (lib trs_jack) (part TRRS_SW_JACK))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C2C6))
    (comp (ref C6)
      (value 2U2)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM188R61C225KE15D))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C687))
    (comp (ref C10)
      (value 2U2)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM188R61C225KE15D))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C68D))
    (comp (ref C3)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C69F))
    (comp (ref C2)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6A5))
    (comp (ref C5)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6AB))
    (comp (ref C4)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6B1))
    (comp (ref C12)
      (value 2U2)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM188R61C225KE15D))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6F0))
    (comp (ref C8)
      (value 2U2)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM188R61C225KE15D))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C6F6))
    (comp (ref C7)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C70E))
    (comp (ref C13)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19)
        (field (name DNP) DNP))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C720))
    (comp (ref C11)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 53A8C72C))
    (comp (ref U1)
      (value AK4951EN)
      (footprint ipc_qfn:IPC_QFN33P40_400X400X80L35X20T280N)
      (datasheet http://www.akm.com/akm/en/file/datasheet/AK4951EN.pdf)
      (fields
        (field (name Mfr) "Asahi Kasei")
        (field (name Part) AK4951EN))
      (libsource (lib asahi_kasei) (part AK4951EN))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58CC98F8))
    (comp (ref R2)
      (value R)
      (footprint ipc_resc:IPC_RESC1608X55L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58CF5E5F))
    (comp (ref U5)
      (value NUF4220MN)
      (footprint ipc_son:IPC_SON9P50_200X200X100L30X25T80X120N)
      (datasheet http://www.onsemi.com/pub/Collateral/NUF4220MN-D.PDF)
      (fields
        (field (name Mfr) "ON Semiconductor")
        (field (name Part) NUF4220MNT1G))
      (libsource (lib on_semi) (part NUF4220MN))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58D9A047))
    (comp (ref TP1)
      (value TP)
      (footprint tp:TP_1MM)
      (libsource (lib tp) (part TP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58EDDA01))
    (comp (ref TP2)
      (value TP)
      (footprint tp:TP_1MM)
      (libsource (lib tp) (part TP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58EDDAEE))
    (comp (ref TP3)
      (value TP)
      (footprint tp:TP_1MM)
      (libsource (lib tp) (part TP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58EDDB69))
    (comp (ref TP4)
      (value TP)
      (footprint tp:TP_1MM)
      (libsource (lib tp) (part TP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58EDDC3F))
    (comp (ref TP5)
      (value TP)
      (footprint tp:TP_1MM)
      (libsource (lib tp) (part TP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58EDDCA8))
    (comp (ref TP6)
      (value TP)
      (footprint tp:TP_1MM)
      (libsource (lib tp) (part TP))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58EDDD10))
    (comp (ref J1)
      (value HEADER_1X3)
      (footprint jst:JST_S3B-PH-SM4-TB)
      (datasheet http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
      (fields
        (field (name Mfr) JST)
        (field (name Part) S3B-PH-SM4-TB)
        (field (name DNP) DNP))
      (libsource (lib header) (part HEADER_1X3))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58F82DA0))
    (comp (ref RP1)
      (value 220R)
      (footprint ipc_resc:IPC_RESCAXS8P80_320X160X60L30X45N)
      (datasheet https://industrial.panasonic.com/cdbs/www-data/pdf/AOC0000/AOC0000C14.pdf)
      (fields
        (field (name Mfr) Panasonic)
        (field (name Part) EXB-38V221JV))
      (libsource (lib passive) (part RPACK4))
      (sheetpath (names /audio/) (tstamps /53A8BFC3/))
      (tstamp 58F9564A))
    (comp (ref R19)
      (value 10K)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name DNP) DNP)
        (field (name Mfr) Yageo))
      (libsource (lib passive) (part R))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A91657))
    (comp (ref J2)
      (value MICROSD_DETSW)
      (footprint alps:ALPS_SCHA4B0419)
      (datasheet http://www.mouser.com/ds/2/15/alps_SCHA4B0419-780241.pdf)
      (fields
        (field (name Mfr) ALPS)
        (field (name Part) SCHA4B0419))
      (libsource (lib sd) (part MICROSD_DETSW))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A8C6D0))
    (comp (ref C27)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53AA73CE))
    (comp (ref SW1)
      (value CK_TSWB-3N-CB)
      (footprint ck:CK_TSWB-3N-CB222_LFS)
      (datasheet http://www.ckswitches.com/media/1346/tsw.pdf)
      (fields
        (field (name Mfr) C&K)
        (field (name Part) "TSWB-3N-CB222 LFS"))
      (libsource (lib ck) (part CK_TSWB-3N-CB))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A8C6FD))
    (comp (ref C26)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 53A8C71C))
    (comp (ref LCD1)
      (value ER-TFT024-3_PANEL)
      (footprint eastrising:ER-TFT024-3)
      (datasheet http://www.buydisplay.com/download/manual/ER-TFT024-3_Datasheet.pdf)
      (fields
        (field (name Mfr) EastRising)
        (field (name Part) ER-TFT024-3))
      (libsource (lib eastrising) (part ER-TFT024-3_PANEL))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 58A60E03))
    (comp (ref J3)
      (value ER-TFT024-3_FPC)
      (footprint eastrising:ER-CON50HT-1)
      (datasheet http://www.buydisplay.com/download/connector/ER-CON50HT-1.pdf)
      (fields
        (field (name Mfr) EastRising)
        (field (name Part) ER-CON50HT-1))
      (libsource (lib eastrising) (part ER-TFT024-3_FPC))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 58AE3A81))
    (comp (ref U4)
      (value CAT4004[_AB])
      (footprint ipc_son:IPC_SON9P50_200X200X55L32X24T90X160N)
      (datasheet http://www.onsemi.com/pub/Collateral/CAT4003B-D.PDF)
      (fields
        (field (name Mfr) "ON Semiconductor")
        (field (name Part) CAT4004BHU2−GT3))
      (libsource (lib on_semi) (part CAT4004[_AB]))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 58B747DD))
    (comp (ref R20)
      (value 3K9)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name DNP) DNP)
        (field (name Mfr) Yageo))
      (libsource (lib passive) (part R))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 58B751E2))
    (comp (ref C14)
      (value 1U)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM188R61C105KA93D))
      (libsource (lib passive) (part C))
      (sheetpath (names /lcd_sw_sd/) (tstamps /53A9129D/))
      (tstamp 58D0DFA2))
    (comp (ref P20)
      (value HACKRF_ONE_P20)
      (footprint header:HEADER_11X2_REV_SM_254_AP)
      (datasheet https://s3.amazonaws.com/mle-assets/parts/TSHSM-1/TSHSM-1.pdf)
      (fields
        (field (name Mfr) MLE)
        (field (name Part) TSHSM-111-D-06-T-V-S-P-TR-AP-LF))
      (libsource (lib hackrf_expansion) (part HACKRF_ONE_P20))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8CDAE))
    (comp (ref P22)
      (value HACKRF_ONE_P22)
      (footprint header:HEADER_13X2_REV_SM_254_AP)
      (datasheet https://s3.amazonaws.com/mle-assets/parts/TSHSM-1/TSHSM-1.pdf)
      (fields
        (field (name Mfr) MLE)
        (field (name Part) TSHSM-113-D-06-T-V-S-P-TR-AP-LF))
      (libsource (lib hackrf_expansion) (part HACKRF_ONE_P22))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8CDB6))
    (comp (ref P28)
      (value HACKRF_ONE_P28)
      (footprint header:HEADER_11X2_REV_SM_254_AP)
      (datasheet https://s3.amazonaws.com/mle-assets/parts/TSHSM-1/TSHSM-1.pdf)
      (fields
        (field (name Mfr) MLE)
        (field (name Part) TSHSM-111-D-06-T-V-S-P-TR-AP-LF))
      (libsource (lib hackrf_expansion) (part HACKRF_ONE_P28))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8CDBE))
    (comp (ref U3)
      (value 5M40ZE64)
      (footprint ipc_qfp:IPC_QFP65P40_900X900X120L60X18T450N)
      (datasheet https://www.altera.com/content/dam/altera-www/global/en_US/pdfs/literature/packaging/04r00384-01.pdf)
      (fields
        (field (name Mfr) Altera)
        (field (name Part) 5M40ZE64C5N))
      (libsource (lib altera) (part 5M40ZE64))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D11B))
    (comp (ref C28)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D527))
    (comp (ref C30)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D542))
    (comp (ref C29)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D548))
    (comp (ref C31)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D54E))
    (comp (ref C33)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D56C))
    (comp (ref C35)
      (value 100N)
      (footprint ipc_capc:IPC_CAPC1005X55L25N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM155R61A104KA01))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D572))
    (comp (ref C32)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5C2))
    (comp (ref C34)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5C8))
    (comp (ref C36)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5DA))
    (comp (ref C37)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53A8D5E0))
    (comp (ref C42)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53B1911F))
    (comp (ref C43)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /hackrf_if/) (tstamps /53A8C780/))
      (tstamp 53B1A065))
    (comp (ref U2)
      (value "TCR2EF18,LM(CT")
      (footprint ipc_sot:IPC_SOT23-5P95_275X135L40X40N)
      (datasheet http://toshiba.semicon-storage.com/ap-en/product/linear/power-supply/detail.TCR2EF18.html)
      (fields
        (field (name Mfr) Toshiba)
        (field (name Part) "TCR2EF18,LM(CT"))
      (libsource (lib regulator) (part REGULATOR_SOT23_5))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58CFF91A))
    (comp (ref C38)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58CFF923))
    (comp (ref C40)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19))
      (libsource (lib passive) (part C))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58CFF92C))
    (comp (ref C39)
      (value R)
      (footprint ipc_capc:IPC_CAPC1608X90L35N)
      (fields
        (field (name DNP) DNP))
      (libsource (lib passive) (part C))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58CFF945))
    (comp (ref BT1)
      (value BATTERY)
      (footprint bat_coin:MPD_BU2032SM-BT-G)
      (datasheet http://www.memoryprotectiondevices.com/datasheets/BU2032SM-BT-GTR-datasheet.pdf)
      (fields
        (field (name Mfr) MPD)
        (field (name Part) BU2032SM-BT-GTR))
      (libsource (lib battery) (part BATTERY))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58D008D0))
    (comp (ref C41)
      (value 10U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name Part) GRM21BR61A106KE19)
        (field (name DNP) DNP))
      (libsource (lib passive) (part C))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58D008E2))
    (comp (ref U6)
      (value BQ24075RGT)
      (footprint ipc_qfn:IPC_QFN17P50_300X300X100L40X25T160N)
      (datasheet http://www.ti.com/lit/ds/symlink/bq24075.pdf)
      (fields
        (field (name Mfr) "Texas Instruments")
        (field (name Part) BQ24075RGT)
        (field (name DNP) DNP))
      (libsource (lib ti) (part BQ24075))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1AA75))
    (comp (ref C1)
      (value 1U)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name DNP) DNP)
        (field (name WVDC) >26V))
      (libsource (lib passive) (part C))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1AC44))
    (comp (ref C16)
      (value 4U7)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name DNP) DNP))
      (libsource (lib passive) (part C))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1AE50))
    (comp (ref C15)
      (value 4U7)
      (footprint ipc_capc:IPC_CAPC2012X135L45N)
      (fields
        (field (name Mfr) Murata)
        (field (name DNP) DNP))
      (libsource (lib passive) (part C))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1B1AB))
    (comp (ref R1)
      (value R)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1CB6B))
    (comp (ref R4)
      (value 1K91)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1CBFA))
    (comp (ref R6)
      (value 1K8)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1CC38))
    (comp (ref R3)
      (value 1K5)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1D0EB))
    (comp (ref R5)
      (value 1K5)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1D207))
    (comp (ref J4)
      (value HEADER_1X2)
      (footprint jst:JST_S2B-PH-SM4-TB)
      (datasheet http://www.jst-mfg.com/product/pdf/eng/ePH.pdf)
      (fields
        (field (name Mfr) JST)
        (field (name Part) S2B-PH-SM4-TB)
        (field (name DNP) DNP))
      (libsource (lib header) (part HEADER_1X2))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1DD77))
    (comp (ref R8)
      (value 10K)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1E372))
    (comp (ref R7)
      (value 0R)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F1F0EF))
    (comp (ref R9)
      (value 10K)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F443CF))
    (comp (ref R10)
      (value 10K)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F44562))
    (comp (ref R14)
      (value 10K)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F44903))
    (comp (ref R13)
      (value 10K)
      (footprint ipc_resc:IPC_RESC1005X40L25N)
      (fields
        (field (name Mfr) Yageo)
        (field (name DNP) DNP))
      (libsource (lib passive) (part R))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F4495E))
    (comp (ref D1)
      (value "LED 0603 green")
      (footprint ipc_ledc:IPC_LEDC1608X90L40N)
      (fields
        (field (name Mfr) Kingbright)
        (field (name Part) APT1608SGC)
        (field (name DNP) DNP))
      (libsource (lib diode) (part LED))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F5B932))
    (comp (ref D2)
      (value "LED 0603 yellow")
      (footprint ipc_ledc:IPC_LEDC1608X90L40N)
      (fields
        (field (name Mfr) Kingbright)
        (field (name Part) APT1608SYCK)
        (field (name DNP) DNP))
      (libsource (lib diode) (part LED))
      (sheetpath (names /power/) (tstamps /58CFF3E3/))
      (tstamp 58F5BA0B)))
  (libparts
    (libpart (lib altera) (part 5M40ZE64)
      (footprints
        (fp IPC_QFP65P40_900X900X120L60X18T450N))
      (fields
        (field (name Reference) U)
        (field (name Value) 5M40ZE64))
      (pins
        (pin (num 1) (name IO/DIFFIO_L1n) (type BiDi))
        (pin (num 2) (name IO) (type BiDi))
        (pin (num 3) (name IO/DIFFIO_L2p) (type BiDi))
        (pin (num 4) (name IO/DIFFIO_L2n) (type BiDi))
        (pin (num 5) (name IO) (type BiDi))
        (pin (num 6) (name VCCIO1) (type power_in))
        (pin (num 7) (name IO/CLK0) (type BiDi))
        (pin (num 8) (name VCCINT) (type power_in))
        (pin (num 9) (name IO/CLK1) (type BiDi))
        (pin (num 10) (name IO) (type BiDi))
        (pin (num 11) (name IO/DIFFIO_L3p) (type BiDi))
        (pin (num 12) (name IO/DIFFIO_L3n) (type BiDi))
        (pin (num 13) (name IO) (type BiDi))
        (pin (num 14) (name TMS) (type input))
        (pin (num 15) (name TDI) (type input))
        (pin (num 16) (name TCK) (type input))
        (pin (num 17) (name TDO) (type output))
        (pin (num 18) (name IO/DIFFIO_B1p) (type BiDi))
        (pin (num 19) (name IO/DIFFIO_B1n) (type BiDi))
        (pin (num 20) (name IO/DIFFIO_B2p) (type BiDi))
        (pin (num 21) (name IO/DIFFIO_B2n) (type BiDi))
        (pin (num 22) (name IO/DIFFIO_B3p) (type BiDi))
        (pin (num 23) (name VCCIO1) (type power_in))
        (pin (num 24) (name IO/DIFFIO_B3n) (type BiDi))
        (pin (num 25) (name IO) (type BiDi))
        (pin (num 26) (name IO/DIFFIO_B4p) (type BiDi))
        (pin (num 27) (name IO/DIFFIO_B4n) (type BiDi))
        (pin (num 28) (name IO/DEV_OE/DIFFIO_B5p) (type BiDi))
        (pin (num 29) (name IO/DEV_CLRn/DIFFIO_B5n) (type BiDi))
        (pin (num 30) (name IO/DIFFIO_B6p) (type BiDi))
        (pin (num 31) (name IO/DIFFIO_B6n) (type BiDi))
        (pin (num 32) (name IO/DIFFIO_B7p) (type BiDi))
        (pin (num 33) (name IO/DIFFIO_B7n) (type BiDi))
        (pin (num 34) (name IO/DIFFIO_R4n) (type BiDi))
        (pin (num 35) (name IO/DIFFIO_R4p) (type BiDi))
        (pin (num 36) (name IO/DIFFIO_R3n) (type BiDi))
        (pin (num 37) (name IO/DIFFIO_R3p) (type BiDi))
        (pin (num 38) (name IO) (type BiDi))
        (pin (num 39) (name VCCIO2) (type power_in))
        (pin (num 40) (name IO/CLK2) (type BiDi))
        (pin (num 41) (name VCCINT) (type power_in))
        (pin (num 42) (name IO/CLK3) (type BiDi))
        (pin (num 43) (name IO/DIFFIO_R2n) (type BiDi))
        (pin (num 44) (name IO/DIFFIO_R2p) (type BiDi))
        (pin (num 45) (name IO) (type BiDi))
        (pin (num 46) (name IO/DIFFIO_R1n) (type BiDi))
        (pin (num 47) (name IO/DIFFIO_R1p) (type BiDi))
        (pin (num 48) (name IO) (type BiDi))
        (pin (num 49) (name IO/DIFFIO_T6n) (type BiDi))
        (pin (num 50) (name IO/DIFFIO_T6p) (type BiDi))
        (pin (num 51) (name IO) (type BiDi))
        (pin (num 52) (name IO/DIFFIO_T5n) (type BiDi))
        (pin (num 53) (name IO/DIFFIO_T5p) (type BiDi))
        (pin (num 54) (name IO/DIFFIO_T4n) (type BiDi))
        (pin (num 55) (name IO/DIFFIO_T4p) (type BiDi))
        (pin (num 56) (name IO/DIFFIO_T3n) (type BiDi))
        (pin (num 57) (name VCCIO2) (type power_in))
        (pin (num 58) (name IO/DIFFIO_T3p) (type BiDi))
        (pin (num 59) (name IO/DIFFIO_T2n) (type BiDi))
        (pin (num 60) (name IO/DIFFIO_T2p) (type BiDi))
        (pin (num 61) (name IO/DIFFIO_T1n) (type BiDi))
        (pin (num 62) (name IO) (type BiDi))
        (pin (num 63) (name IO/DIFFIO_T1p) (type BiDi))
        (pin (num 64) (name IO/DIFFIO_L1p) (type BiDi))
        (pin (num 65) (name GND) (type power_in))))
    (libpart (lib asahi_kasei) (part AK4951EN)
      (footprints
        (fp IPC_QFN33P40_400X400X80L35X20T280N))
      (fields
        (field (name Reference) U)
        (field (name Value) AK4951EN))
      (pins
        (pin (num 1) (name LIN3) (type input))
        (pin (num 2) (name RIN2) (type input))
        (pin (num 3) (name LIN2) (type input))
        (pin (num 4) (name MPWR2) (type output))
        (pin (num 5) (name MPWR1) (type output))
        (pin (num 6) (name RIN1/DMCLK) (type BiDi))
        (pin (num 7) (name LIN1/DMDAT) (type input))
        (pin (num 8) (name PDN) (type input))
        (pin (num 9) (name SCL) (type input))
        (pin (num 10) (name SDA) (type BiDi))
        (pin (num 11) (name SDTI) (type input))
        (pin (num 12) (name SDTO) (type output))
        (pin (num 13) (name LRCK) (type BiDi))
        (pin (num 14) (name BICK) (type BiDi))
        (pin (num 15) (name MCKI) (type input))
        (pin (num 16) (name TVDD) (type power_in))
        (pin (num 17) (name VSS3) (type power_in))
        (pin (num 18) (name SVDD) (type power_in))
        (pin (num 19) (name SPN/ROUT) (type output))
        (pin (num 20) (name SPP/LOUT) (type output))
        (pin (num 21) (name DVDD) (type power_in))
        (pin (num 22) (name HPL) (type output))
        (pin (num 23) (name HPR) (type output))
        (pin (num 24) (name VEE) (type output))
        (pin (num 25) (name VSS2) (type power_in))
        (pin (num 26) (name CP) (type output))
        (pin (num 27) (name CN) (type input))
        (pin (num 28) (name AVDD) (type power_in))
        (pin (num 29) (name VSS1) (type power_in))
        (pin (num 30) (name VCOM) (type output))
        (pin (num 31) (name REGFIL) (type output))
        (pin (num 32) (name RIN3/BEEP) (type input))
        (pin (num 33) (name PAD) (type power_in))))
    (libpart (lib battery) (part BATTERY)
      (footprints
        (fp MPD_BU2032SM-BT-G))
      (fields
        (field (name Reference) BT)
        (field (name Value) BATTERY))
      (pins
        (pin (num 1) (name +) (type power_out))
        (pin (num 2) (name -) (type power_out))))
    (libpart (lib ti) (part BQ24075)
      (footprints
        (fp IPC_QFN17P50_300X300X100L40X25T160N))
      (fields
        (field (name Reference) U)
        (field (name Value) BQ24075))
      (pins
        (pin (num 1) (name TS) (type input))
        (pin (num 2) (name BAT) (type BiDi))
        (pin (num 3) (name BAT) (type BiDi))
        (pin (num 4) (name CE#) (type input))
        (pin (num 5) (name EN2) (type input))
        (pin (num 6) (name EN1) (type input))
        (pin (num 7) (name PGOOD#) (type openCol))
        (pin (num 8) (name VSS) (type power_in))
        (pin (num 9) (name CHG#) (type openCol))
        (pin (num 10) (name OUT) (type power_out))
        (pin (num 11) (name OUT) (type power_out))
        (pin (num 12) (name ILIM) (type input))
        (pin (num 13) (name IN) (type power_in))
        (pin (num 14) (name TMR) (type input))
        (pin (num 15) (name SYSOFF) (type input))
        (pin (num 16) (name ISET) (type BiDi))
        (pin (num 17) (name PAD) (type power_in))))
    (libpart (lib passive) (part C)
      (footprints
        (fp IPC_CAPC*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib on_semi) (part CAT4004[_AB])
      (description "LED Driver, 4 channel")
      (footprints
        (fp IPC_SON9P50_200X200X55L32X24T90X160N))
      (fields
        (field (name Reference) U)
        (field (name Value) CAT4004[_AB]))
      (pins
        (pin (num 1) (name EN/DIM) (type input))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name LED1) (type power_out))
        (pin (num 4) (name LED2) (type power_out))
        (pin (num 5) (name LED3) (type power_out))
        (pin (num 6) (name LED4) (type power_out))
        (pin (num 7) (name RSET/NC) (type passive))
        (pin (num 8) (name VIN) (type power_in))
        (pin (num 9) (name PAD) (type power_in))))
    (libpart (lib ck) (part CK_TSWB-3N-CB)
      (footprints
        (fp CK_TSWB-3N-CB*))
      (fields
        (field (name Reference) SW)
        (field (name Value) CK_TSWB-3N-CB))
      (pins
        (pin (num A) (name ROT_A) (type BiDi))
        (pin (num B) (name ROT_B) (type BiDi))
        (pin (num CA) (name COM_A) (type BiDi))
        (pin (num CB) (name COM_B) (type BiDi))
        (pin (num S1) (name SEL) (type BiDi))
        (pin (num S2) (name D) (type BiDi))
        (pin (num S3) (name R) (type BiDi))
        (pin (num S4) (name U) (type BiDi))
        (pin (num S5) (name L) (type BiDi))))
    (libpart (lib eastrising) (part ER-TFT024-3_FPC)
      (footprints
        (fp ER-CON50HT-1))
      (fields
        (field (name Reference) J)
        (field (name Value) ER-TFT024-3_FPC))
      (pins
        (pin (num 1) (name LEDA) (type power_in))
        (pin (num 2) (name LEDK1) (type power_in))
        (pin (num 3) (name LEDK2) (type power_in))
        (pin (num 4) (name LEDK3) (type power_in))
        (pin (num 5) (name LEDK4) (type power_in))
        (pin (num 6) (name IM0) (type input))
        (pin (num 7) (name IM1) (type input))
        (pin (num 8) (name IM2) (type input))
        (pin (num 9) (name IM3) (type input))
        (pin (num 10) (name RESET) (type input))
        (pin (num 11) (name VSYNC) (type input))
        (pin (num 12) (name HSYNC) (type input))
        (pin (num 13) (name DOTCLK) (type input))
        (pin (num 14) (name DE) (type input))
        (pin (num 15) (name DB17) (type BiDi))
        (pin (num 16) (name DB16) (type BiDi))
        (pin (num 17) (name DB15) (type BiDi))
        (pin (num 18) (name DB14) (type BiDi))
        (pin (num 19) (name DB13) (type BiDi))
        (pin (num 20) (name DB12) (type BiDi))
        (pin (num 21) (name DB11) (type BiDi))
        (pin (num 22) (name DB10) (type BiDi))
        (pin (num 23) (name DB9) (type BiDi))
        (pin (num 24) (name DB8) (type BiDi))
        (pin (num 25) (name DB7) (type BiDi))
        (pin (num 26) (name DB6) (type BiDi))
        (pin (num 27) (name DB5) (type BiDi))
        (pin (num 28) (name DB4) (type BiDi))
        (pin (num 29) (name DB3) (type BiDi))
        (pin (num 30) (name DB2) (type BiDi))
        (pin (num 31) (name DB1) (type BiDi))
        (pin (num 32) (name DB0) (type BiDi))
        (pin (num 33) (name SDO) (type output))
        (pin (num 34) (name SDI) (type input))
        (pin (num 35) (name RD) (type input))
        (pin (num 36) (name "WRX(D/CX)") (type input))
        (pin (num 37) (name "D/CX(SCL)") (type input))
        (pin (num 38) (name CSX) (type input))
        (pin (num 39) (name TE) (type output))
        (pin (num 40) (name VDDI) (type power_in))
        (pin (num 41) (name VDDI) (type power_in))
        (pin (num 42) (name VCI) (type power_in))
        (pin (num 43) (name GND) (type power_in))
        (pin (num 44) (name XP) (type passive))
        (pin (num 45) (name YP) (type passive))
        (pin (num 46) (name XN) (type passive))
        (pin (num 47) (name YN) (type passive))
        (pin (num 48) (name GND) (type power_in))
        (pin (num 49) (name GND) (type power_in))
        (pin (num 50) (name GND) (type power_in))
        (pin (num SHLD) (name ~) (type passive))))
    (libpart (lib eastrising) (part ER-TFT024-3_PANEL)
      (description "2.4\" LCD panel")
      (footprints
        (fp ER-TFT024-3))
      (fields
        (field (name Reference) LCD)
        (field (name Value) ER-TFT024-3_PANEL)))
    (libpart (lib fiducial) (part FIDUCIAL)
      (footprints
        (fp FIDUCIAL_65MIL))
      (fields
        (field (name Reference) FID)
        (field (name Value) FIDUCIAL)))
    (libpart (lib hackrf_expansion) (part HACKRF_ONE_P20)
      (footprints
        (fp HEADER_11X2_*_254))
      (fields
        (field (name Reference) J)
        (field (name Value) HACKRF_ONE_P20))
      (pins
        (pin (num 1) (name VBAT) (type power_in))
        (pin (num 2) (name RTC_ALARM) (type output))
        (pin (num 3) (name VCC) (type power_out))
        (pin (num 4) (name WAKEUP) (type input))
        (pin (num 5) (name GPIO3_8) (type BiDi))
        (pin (num 6) (name GPIO3_9) (type BiDi))
        (pin (num 7) (name GPIO3_10) (type BiDi))
        (pin (num 8) (name GPIO3_11) (type BiDi))
        (pin (num 9) (name GPIO3_12) (type BiDi))
        (pin (num 10) (name GPIO3_13) (type BiDi))
        (pin (num 11) (name GPIO3_14) (type BiDi))
        (pin (num 12) (name GPIO3_15) (type BiDi))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 14) (name ADC0_6) (type input))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name ADC0_2) (type input))
        (pin (num 17) (name VBUSCTRL) (type input))
        (pin (num 18) (name ADC0_5) (type input))
        (pin (num 19) (name GND) (type power_in))
        (pin (num 20) (name ADC0_0) (type input))
        (pin (num 21) (name VBUS) (type output))
        (pin (num 22) (name VIN) (type power_in))))
    (libpart (lib hackrf_expansion) (part HACKRF_ONE_P22)
      (footprints
        (fp HEADER_13X2_*_254))
      (fields
        (field (name Reference) J)
        (field (name Value) HACKRF_ONE_P22))
      (pins
        (pin (num 1) (name CLKOUT) (type output))
        (pin (num 2) (name CLKIN) (type input))
        (pin (num 3) (name RESET#) (type output))
        (pin (num 4) (name GND) (type power_in))
        (pin (num 5) (name I2C1_SCL) (type output))
        (pin (num 6) (name I2C1_SDA) (type BiDi))
        (pin (num 7) (name SPIFI_MISO) (type input))
        (pin (num 8) (name SPIFI_SCK) (type output))
        (pin (num 9) (name SPIFI_MOSI) (type output))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name VCC) (type power_out))
        (pin (num 12) (name I2S0_RX_SCK) (type output))
        (pin (num 13) (name I2S0_RX_SDA) (type input))
        (pin (num 14) (name I2S0_RX_MCLK) (type output))
        (pin (num 15) (name I2S0_RX_WS) (type output))
        (pin (num 16) (name I2S0_TX_SCK) (type output))
        (pin (num 17) (name I2S0_TX_MCLK) (type output))
        (pin (num 18) (name GND) (type power_in))
        (pin (num 19) (name U0_RXD) (type input))
        (pin (num 20) (name U0_TXD) (type output))
        (pin (num 21) (name P2_9) (type BiDi))
        (pin (num 22) (name P2_13) (type BiDi))
        (pin (num 23) (name P2_8) (type BiDi))
        (pin (num 24) (name SDA) (type BiDi))
        (pin (num 25) (name CLK6) (type output))
        (pin (num 26) (name SCL) (type output))))
    (libpart (lib hackrf_expansion) (part HACKRF_ONE_P28)
      (footprints
        (fp HEADER_11X2_*_254))
      (fields
        (field (name Reference) J)
        (field (name Value) HACKRF_ONE_P28))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name SD_CD) (type BiDi))
        (pin (num 4) (name SD_DAT3) (type BiDi))
        (pin (num 5) (name SD_DAT2) (type BiDi))
        (pin (num 6) (name SD_DAT1) (type BiDi))
        (pin (num 7) (name SD_DAT0) (type BiDi))
        (pin (num 8) (name SD_VOLT0) (type BiDi))
        (pin (num 9) (name SD_CMD) (type BiDi))
        (pin (num 10) (name SD_POW) (type BiDi))
        (pin (num 11) (name SD_CLK) (type BiDi))
        (pin (num 12) (name GND) (type power_in))
        (pin (num 13) (name GCLK2) (type output))
        (pin (num 14) (name GCK1) (type output))
        (pin (num 15) (name B1AUX14) (type BiDi))
        (pin (num 16) (name B1AUX13) (type BiDi))
        (pin (num 17) (name CPLD_TCK) (type output))
        (pin (num 18) (name BANK2F3M2) (type BiDi))
        (pin (num 19) (name CPLD_TDI) (type input))
        (pin (num 20) (name BANK2F3M6) (type BiDi))
        (pin (num 21) (name BANK2F3M12) (type BiDi))
        (pin (num 22) (name BANK2F3M4) (type BiDi))))
    (libpart (lib header) (part HEADER_1X2)
      (footprints
        (fp JST_S2B-PH-SM4-TB))
      (fields
        (field (name Reference) J)
        (field (name Value) HEADER_1X2))
      (pins
        (pin (num 1) (name ~) (type unspc))
        (pin (num 2) (name ~) (type unspc))))
    (libpart (lib header) (part HEADER_1X3)
      (fields
        (field (name Reference) J)
        (field (name Value) HEADER_1X3))
      (pins
        (pin (num 1) (name ~) (type unspc))
        (pin (num 2) (name ~) (type unspc))
        (pin (num 3) (name ~) (type unspc))))
    (libpart (lib hole) (part HOLE1)
      (footprints
        (fp *HOLE*))
      (fields
        (field (name Reference) H)
        (field (name Value) HOLE1))
      (pins
        (pin (num 1) (name ~) (type passive))))
    (libpart (lib diode) (part LED)
      (footprints
        (fp IPC_LEDC*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num A) (name A) (type passive))
        (pin (num C) (name K) (type passive))))
    (libpart (lib sd) (part MICROSD_DETSW)
      (footprints
        (fp HIROSE_DM3D)
        (fp ALPS_SCHA4B0400)
        (fp ALPS_SCHA4B0419))
      (fields
        (field (name Reference) J)
        (field (name Value) MICROSD_DETSW))
      (pins
        (pin (num 0) (name GND) (type power_in))
        (pin (num 1) (name DAT2) (type BiDi))
        (pin (num 2) (name DAT3/CD) (type BiDi))
        (pin (num 3) (name CMD) (type BiDi))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name CLK) (type input))
        (pin (num 6) (name VSS) (type power_in))
        (pin (num 7) (name DAT0) (type BiDi))
        (pin (num 8) (name DAT1) (type BiDi))
        (pin (num A) (name DETA) (type passive))
        (pin (num B) (name DETB) (type passive))
        (pin (num SH) (name SHIELD) (type passive))))
    (libpart (lib on_semi) (part NUF4220MN)
      (footprints
        (fp IPC_SON9P50_200X200X100L30X25T80X120N))
      (fields
        (field (name Reference) U)
        (field (name Value) NUF4220MN))
      (pins
        (pin (num 1) (name C1A) (type passive))
        (pin (num 2) (name C2A) (type passive))
        (pin (num 3) (name C3A) (type passive))
        (pin (num 4) (name C4A) (type passive))
        (pin (num 5) (name C4B) (type passive))
        (pin (num 6) (name C3B) (type passive))
        (pin (num 7) (name C2B) (type passive))
        (pin (num 8) (name C1B) (type passive))
        (pin (num 9) (name GND) (type power_in))))
    (libpart (lib passive) (part R)
      (footprints
        (fp IPC_RESC*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib regulator) (part REGULATOR_SOT23_5)
      (footprints
        (fp IPC_SOT23-5P95_275X135L40X40N))
      (fields
        (field (name Reference) U)
        (field (name Value) REGULATOR_SOT23_5))
      (pins
        (pin (num 1) (name VIN) (type power_in))
        (pin (num 2) (name GND) (type power_in))
        (pin (num 3) (name EN) (type input))
        (pin (num 4) (name BP) (type input))
        (pin (num 5) (name VOUT) (type power_out))))
    (libpart (lib passive) (part RPACK4)
      (footprints
        (fp IPC_RESCAXS80P160X320X60-8N)
        (fp IPC_RESCAXS8P80_320X160X60L30X45N))
      (fields
        (field (name Reference) RP)
        (field (name Value) RPACK4))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))
        (pin (num 3) (name ~) (type passive))
        (pin (num 4) (name ~) (type passive))
        (pin (num 5) (name ~) (type passive))
        (pin (num 6) (name ~) (type passive))
        (pin (num 7) (name ~) (type passive))
        (pin (num 8) (name ~) (type passive))))
    (libpart (lib tp) (part TP)
      (footprints
        (fp TP_*))
      (fields
        (field (name Reference) TP)
        (field (name Value) TP))
      (pins
        (pin (num 1) (name TP) (type passive))))
    (libpart (lib trs_jack) (part TRRS_SW_JACK)
      (footprints
        (fp CUI_SJ-43516-SMT))
      (fields
        (field (name Reference) P)
        (field (name Value) TRRS_SW_JACK))
      (pins
        (pin (num 1) (name S) (type passive))
        (pin (num 2) (name T) (type passive))
        (pin (num 3) (name R1) (type passive))
        (pin (num 4) (name R2) (type passive))
        (pin (num 5) (name TSW) (type passive))
        (pin (num 6) (name RSW) (type passive)))))
  (libraries
    (library (logical trs_jack)
      (uri /home/jboone/src/library-kicad/trs_jack.lib))
    (library (logical battery)
      (uri /home/jboone/src/library-kicad/battery.lib))
    (library (logical ck)
      (uri /home/jboone/src/library-kicad/ck.lib))
    (library (logical asahi_kasei)
      (uri /home/jboone/src/library-kicad/asahi_kasei.lib))
    (library (logical header)
      (uri /home/jboone/src/library-kicad/header.lib))
    (library (logical passive)
      (uri /home/jboone/src/library-kicad/passive.lib))
    (library (logical on_semi)
      (uri /home/jboone/src/library-kicad/on_semi.lib))
    (library (logical tp)
      (uri /home/jboone/src/library-kicad/tp.lib))
    (library (logical sd)
      (uri /home/jboone/src/library-kicad/sd.lib))
    (library (logical hackrf_expansion)
      (uri /home/jboone/src/library-kicad/hackrf_expansion.lib))
    (library (logical altera)
      (uri /home/jboone/src/library-kicad/altera.lib))
    (library (logical fiducial)
      (uri /home/jboone/src/library-kicad/fiducial.lib))
    (library (logical ti)
      (uri /home/jboone/src/library-kicad/ti.lib))
    (library (logical hole)
      (uri /home/jboone/src/library-kicad/hole.lib))
    (library (logical diode)
      (uri /home/jboone/src/library-kicad/diode.lib))
    (library (logical regulator)
      (uri /home/jboone/src/library-kicad/regulator.lib))
    (library (logical eastrising)
      (uri /home/jboone/src/library-kicad/eastrising.lib)))
  (nets
    (net (code 1) (name /hackrf_if/SW_R)
      (node (ref SW1) (pin S3))
      (node (ref U3) (pin 9)))
    (net (code 2) (name /hackrf_if/LCD_BACKLIGHT)
      (node (ref U3) (pin 37))
      (node (ref U4) (pin 1)))
    (net (code 3) (name /hackrf_if/LCD_RESET#)
      (node (ref R19) (pin 1))
      (node (ref U3) (pin 38))
      (node (ref J3) (pin 10)))
    (net (code 4) (name /hackrf_if/LCD_RS)
      (node (ref U3) (pin 62))
      (node (ref J3) (pin 37)))
    (net (code 5) (name /hackrf_if/LCD_RD#)
      (node (ref U3) (pin 60))
      (node (ref J3) (pin 35)))
    (net (code 6) (name /hackrf_if/LCD_WR#)
      (node (ref U3) (pin 61))
      (node (ref J3) (pin 36)))
    (net (code 7) (name /hackrf_if/LCD_TE)
      (node (ref J3) (pin 39))
      (node (ref U3) (pin 63)))
    (net (code 8) (name /hackrf_if/TP_U)
      (node (ref J3) (pin 47))
      (node (ref U3) (pin 3))
      (node (ref P20) (pin 20)))
    (net (code 9) (name /hackrf_if/TP_R)
      (node (ref U3) (pin 64))
      (node (ref J3) (pin 44))
      (node (ref P20) (pin 14)))
    (net (code 10) (name /hackrf_if/TP_D)
      (node (ref J3) (pin 45))
      (node (ref P20) (pin 16))
      (node (ref U3) (pin 1)))
    (net (code 11) (name /hackrf_if/TP_L)
      (node (ref J3) (pin 46))
      (node (ref P20) (pin 18))
      (node (ref U3) (pin 2)))
    (net (code 12) (name /hackrf_if/SW_U)
      (node (ref SW1) (pin S4))
      (node (ref U3) (pin 25)))
    (net (code 13) (name /hackrf_if/SW_D)
      (node (ref U3) (pin 10))
      (node (ref SW1) (pin S2)))
    (net (code 14) (name /hackrf_if/SW_L)
      (node (ref SW1) (pin S5))
      (node (ref U3) (pin 28)))
    (net (code 15) (name /hackrf_if/SW_ROT_A)
      (node (ref U3) (pin 11))
      (node (ref SW1) (pin A)))
    (net (code 16) (name /hackrf_if/SW_ROT_B)
      (node (ref U3) (pin 12))
      (node (ref SW1) (pin B)))
    (net (code 17) (name /hackrf_if/SW_SEL)
      (node (ref SW1) (pin S1))
      (node (ref U3) (pin 13)))
    (net (code 18) (name /hackrf_if/SD_CD)
      (node (ref J2) (pin B))
      (node (ref P28) (pin 3)))
    (net (code 19) (name /hackrf_if/SD_CLK)
      (node (ref P28) (pin 11))
      (node (ref J2) (pin 5)))
    (net (code 20) (name /hackrf_if/SD_CMD)
      (node (ref J2) (pin 3))
      (node (ref P28) (pin 9)))
    (net (code 21) (name /hackrf_if/SD_DAT0)
      (node (ref J2) (pin 7))
      (node (ref P28) (pin 7)))
    (net (code 22) (name /hackrf_if/SD_DAT1)
      (node (ref P28) (pin 6))
      (node (ref J2) (pin 8)))
    (net (code 23) (name /hackrf_if/SD_DAT2)
      (node (ref J2) (pin 1))
      (node (ref P28) (pin 5)))
    (net (code 24) (name GND)
      (node (ref U1) (pin 33))
      (node (ref SW1) (pin CB))
      (node (ref U1) (pin 17))
      (node (ref J3) (pin 13))
      (node (ref U1) (pin 25))
      (node (ref J2) (pin 0))
      (node (ref C10) (pin 1))
      (node (ref J2) (pin A))
      (node (ref C3) (pin 2))
      (node (ref U1) (pin 29))
      (node (ref J2) (pin 6))
      (node (ref P20) (pin 19))
      (node (ref R19) (pin 2))
      (node (ref C27) (pin 2))
      (node (ref U5) (pin 9))
      (node (ref R2) (pin 2))
      (node (ref U5) (pin 2))
      (node (ref C26) (pin 2))
      (node (ref SW1) (pin CA))
      (node (ref J2) (pin SH))
      (node (ref C43) (pin 2))
      (node (ref P22) (pin 4))
      (node (ref P28) (pin 12))
      (node (ref P22) (pin 10))
      (node (ref P28) (pin 2))
      (node (ref P22) (pin 18))
      (node (ref C42) (pin 2))
      (node (ref U3) (pin 65))
      (node (ref C35) (pin 2))
      (node (ref C33) (pin 2))
      (node (ref J3) (pin 7))
      (node (ref P20) (pin 13))
      (node (ref P20) (pin 15))
      (node (ref C32) (pin 2))
      (node (ref J3) (pin 14))
      (node (ref J3) (pin 34))
      (node (ref J3) (pin 15))
      (node (ref J3) (pin 16))
      (node (ref J3) (pin 43))
      (node (ref J3) (pin 38))
      (node (ref J3) (pin 8))
      (node (ref J3) (pin 9))
      (node (ref J3) (pin 50))
      (node (ref J3) (pin 11))
      (node (ref C29) (pin 2))
      (node (ref C37) (pin 2))
      (node (ref C36) (pin 2))
      (node (ref C28) (pin 2))
      (node (ref C30) (pin 2))
      (node (ref J3) (pin 12))
      (node (ref C31) (pin 2))
      (node (ref C34) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref J1) (pin 2))
      (node (ref R6) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref H2) (pin 1))
      (node (ref R14) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref J4) (pin 2))
      (node (ref R8) (pin 2))
      (node (ref H3) (pin 1))
      (node (ref H5) (pin 1))
      (node (ref H4) (pin 1))
      (node (ref U6) (pin 17))
      (node (ref C1) (pin 2))
      (node (ref BT1) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R10) (pin 2))
      (node (ref C39) (pin 2))
      (node (ref C41) (pin 2))
      (node (ref U6) (pin 8))
      (node (ref U2) (pin 2))
      (node (ref C38) (pin 2))
      (node (ref C40) (pin 2))
      (node (ref C12) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref U4) (pin 9))
      (node (ref C8) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref J3) (pin 49))
      (node (ref J3) (pin SHLD))
      (node (ref C2) (pin 2))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 2))
      (node (ref R11) (pin 2))
      (node (ref R12) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref J3) (pin 48))
      (node (ref U4) (pin 2))
      (node (ref R20) (pin 2)))
    (net (code 25) (name /hackrf_if/AUDIO_RESET#)
      (node (ref RP1) (pin 5))
      (node (ref U3) (pin 4)))
    (net (code 26) (name /hackrf_if/I2S0_WS)
      (node (ref P22) (pin 15))
      (node (ref RP1) (pin 7)))
    (net (code 27) (name /audio/BICK)
      (node (ref RP1) (pin 8))
      (node (ref P22) (pin 16)))
    (net (code 28) (name /hackrf_if/VBUSCTRL)
      (node (ref P20) (pin 17))
      (node (ref R7) (pin 2)))
    (net (code 29) (name /hackrf_if/VBUS)
      (node (ref U6) (pin 13))
      (node (ref C1) (pin 1))
      (node (ref P20) (pin 21))
      (node (ref R7) (pin 1)))
    (net (code 30) (name /hackrf_if/VBAT)
      (node (ref BT1) (pin 1))
      (node (ref C41) (pin 1))
      (node (ref P20) (pin 1)))
    (net (code 31) (name /power/AUDIO_SVDD)
      (node (ref C16) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref R13) (pin 1))
      (node (ref U6) (pin 10))
      (node (ref U6) (pin 11))
      (node (ref U1) (pin 18))
      (node (ref C13) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref P20) (pin 22)))
    (net (code 32) (name +3.3V)
      (node (ref C42) (pin 1))
      (node (ref C34) (pin 1))
      (node (ref C32) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref J3) (pin 1))
      (node (ref C43) (pin 1))
      (node (ref C27) (pin 1))
      (node (ref P28) (pin 1))
      (node (ref P22) (pin 11))
      (node (ref J3) (pin 42))
      (node (ref U1) (pin 16))
      (node (ref C38) (pin 1))
      (node (ref J2) (pin 4))
      (node (ref U1) (pin 28))
      (node (ref U2) (pin 3))
      (node (ref C28) (pin 1))
      (node (ref C26) (pin 1))
      (node (ref C30) (pin 1))
      (node (ref P20) (pin 3))
      (node (ref U3) (pin 23))
      (node (ref U4) (pin 8))
      (node (ref U3) (pin 6))
      (node (ref C7) (pin 1))
      (node (ref U2) (pin 1)))
    (net (code 33) (name +1.8V)
      (node (ref C35) (pin 1))
      (node (ref C33) (pin 1))
      (node (ref C37) (pin 1))
      (node (ref C36) (pin 1))
      (node (ref U3) (pin 39))
      (node (ref U3) (pin 57))
      (node (ref C29) (pin 1))
      (node (ref C31) (pin 1))
      (node (ref C3) (pin 1))
      (node (ref J3) (pin 6))
      (node (ref U3) (pin 41))
      (node (ref J3) (pin 41))
      (node (ref J3) (pin 40))
      (node (ref U3) (pin 8))
      (node (ref U2) (pin 5))
      (node (ref C40) (pin 1))
      (node (ref U1) (pin 21)))
    (net (code 34) (name /hackrf_if/SD_DAT3)
      (node (ref P28) (pin 4))
      (node (ref J2) (pin 2)))
    (net (code 35) (name /hackrf_if/I2S0_MCLK)
      (node (ref P22) (pin 17))
      (node (ref U1) (pin 15)))
    (net (code 36) (name /hackrf_if/I2S0_TX_SDA)
      (node (ref U1) (pin 11))
      (node (ref P22) (pin 13)))
    (net (code 37) (name /hackrf_if/I2S0_RX_SDA)
      (node (ref RP1) (pin 6))
      (node (ref U3) (pin 15))
      (node (ref P28) (pin 19)))
    (net (code 38) (name /audio/SCL)
      (node (ref U1) (pin 9))
      (node (ref P22) (pin 26)))
    (net (code 39) (name /audio/SDA)
      (node (ref P22) (pin 24))
      (node (ref U1) (pin 10)))
    (net (code 40) (name "Net-(C25-Pad1)")
      (node (ref U1) (pin 3))
      (node (ref C25) (pin 1)))
    (net (code 41) (name "Net-(R18-Pad1)")
      (node (ref U1) (pin 4))
      (node (ref R18) (pin 1)))
    (net (code 42) (name "Net-(TP4-Pad1)")
      (node (ref U1) (pin 5))
      (node (ref TP4) (pin 1)))
    (net (code 43) (name "Net-(TP6-Pad1)")
      (node (ref TP6) (pin 1))
      (node (ref U1) (pin 7)))
    (net (code 44) (name "Net-(TP5-Pad1)")
      (node (ref U1) (pin 6))
      (node (ref TP5) (pin 1)))
    (net (code 45) (name "Net-(TP3-Pad1)")
      (node (ref TP3) (pin 1))
      (node (ref U1) (pin 2)))
    (net (code 46) (name "Net-(TP2-Pad1)")
      (node (ref TP2) (pin 1))
      (node (ref U1) (pin 1)))
    (net (code 47) (name "Net-(TP1-Pad1)")
      (node (ref U1) (pin 32))
      (node (ref TP1) (pin 1)))
    (net (code 48) (name /audio/MIC)
      (node (ref R18) (pin 2))
      (node (ref U5) (pin 3))
      (node (ref C25) (pin 2)))
    (net (code 49) (name /audio/RHPOUT)
      (node (ref U1) (pin 23))
      (node (ref U5) (pin 4))
      (node (ref C23) (pin 1)))
    (net (code 50) (name /audio/LHPOUT)
      (node (ref U5) (pin 1))
      (node (ref C22) (pin 1))
      (node (ref U1) (pin 22)))
    (net (code 51) (name /audio/RHPOUT_X)
      (node (ref U5) (pin 5))
      (node (ref P2) (pin 3)))
    (net (code 52) (name /audio/GND_X)
      (node (ref P2) (pin 4))
      (node (ref U5) (pin 7)))
    (net (code 53) (name "Net-(C23-Pad2)")
      (node (ref C23) (pin 2))
      (node (ref R12) (pin 1)))
    (net (code 54) (name "Net-(C22-Pad2)")
      (node (ref R11) (pin 1))
      (node (ref C22) (pin 2)))
    (net (code 55) (name /audio/SPN)
      (node (ref J1) (pin 1))
      (node (ref U1) (pin 19)))
    (net (code 56) (name /audio/SPP)
      (node (ref U1) (pin 20))
      (node (ref J1) (pin 3)))
    (net (code 57) (name /audio/SDTO_R)
      (node (ref RP1) (pin 3))
      (node (ref U1) (pin 12)))
    (net (code 58) (name /audio/LRCK_R)
      (node (ref U1) (pin 13))
      (node (ref RP1) (pin 2)))
    (net (code 59) (name /audio/BICK_R)
      (node (ref U1) (pin 14))
      (node (ref RP1) (pin 1)))
    (net (code 60) (name /audio/PDN#_R)
      (node (ref R2) (pin 1))
      (node (ref U1) (pin 8))
      (node (ref RP1) (pin 4)))
    (net (code 61) (name "Net-(P2-Pad5)")
      (node (ref P2) (pin 5)))
    (net (code 62) (name "Net-(P2-Pad6)")
      (node (ref P2) (pin 6)))
    (net (code 63) (name /audio/LHPOUT_X)
      (node (ref U5) (pin 8))
      (node (ref P2) (pin 2)))
    (net (code 64) (name /audio/CP)
      (node (ref C6) (pin 1))
      (node (ref U1) (pin 26)))
    (net (code 65) (name /audio/CN)
      (node (ref C6) (pin 2))
      (node (ref U1) (pin 27)))
    (net (code 66) (name /audio/VEE)
      (node (ref C8) (pin 1))
      (node (ref U1) (pin 24)))
    (net (code 67) (name /audio/REGFIL)
      (node (ref C12) (pin 2))
      (node (ref U1) (pin 31)))
    (net (code 68) (name /audio/VCOM)
      (node (ref U1) (pin 30))
      (node (ref C10) (pin 2)))
    (net (code 69) (name /audio/MIC_X)
      (node (ref P2) (pin 1))
      (node (ref U5) (pin 6)))
    (net (code 70) (name "Net-(P22-Pad7)")
      (node (ref P22) (pin 7)))
    (net (code 71) (name "Net-(P22-Pad9)")
      (node (ref P22) (pin 9)))
    (net (code 72) (name "Net-(P22-Pad25)")
      (node (ref P22) (pin 25)))
    (net (code 73) (name "Net-(P28-Pad18)")
      (node (ref P28) (pin 18)))
    (net (code 74) (name "Net-(P28-Pad20)")
      (node (ref P28) (pin 20)))
    (net (code 75) (name "Net-(P28-Pad22)")
      (node (ref P28) (pin 22)))
    (net (code 76) (name "Net-(P28-Pad21)")
      (node (ref P28) (pin 21)))
    (net (code 77) (name /hackrf_if/PP_CPLD_TDO)
      (node (ref U3) (pin 17))
      (node (ref P28) (pin 10)))
    (net (code 78) (name "Net-(P22-Pad8)")
      (node (ref P22) (pin 8)))
    (net (code 79) (name "Net-(P22-Pad1)")
      (node (ref P22) (pin 1)))
    (net (code 80) (name "Net-(P28-Pad13)")
      (node (ref P28) (pin 13)))
    (net (code 81) (name "Net-(P28-Pad14)")
      (node (ref P28) (pin 14)))
    (net (code 82) (name "Net-(P20-Pad4)")
      (node (ref P20) (pin 4)))
    (net (code 83) (name /hackrf_if/MCU_D7)
      (node (ref U3) (pin 18))
      (node (ref P20) (pin 12)))
    (net (code 84) (name /hackrf_if/MCU_D6)
      (node (ref P20) (pin 11))
      (node (ref U3) (pin 19)))
    (net (code 85) (name /hackrf_if/MCU_D5)
      (node (ref U3) (pin 21))
      (node (ref P20) (pin 10)))
    (net (code 86) (name /hackrf_if/MCU_D4)
      (node (ref U3) (pin 20))
      (node (ref P20) (pin 9)))
    (net (code 87) (name /hackrf_if/MCU_D3)
      (node (ref P20) (pin 8))
      (node (ref U3) (pin 22)))
    (net (code 88) (name /hackrf_if/MCU_D2)
      (node (ref P20) (pin 7))
      (node (ref U3) (pin 24)))
    (net (code 89) (name /hackrf_if/MCU_D1)
      (node (ref U3) (pin 27))
      (node (ref P20) (pin 6)))
    (net (code 90) (name /hackrf_if/MCU_D0)
      (node (ref U3) (pin 26))
      (node (ref P20) (pin 5)))
    (net (code 91) (name "Net-(P28-Pad15)")
      (node (ref P28) (pin 15)))
    (net (code 92) (name "Net-(P20-Pad2)")
      (node (ref P20) (pin 2)))
    (net (code 93) (name "Net-(P22-Pad14)")
      (node (ref P22) (pin 14)))
    (net (code 94) (name "Net-(P22-Pad12)")
      (node (ref P22) (pin 12)))
    (net (code 95) (name /hackrf_if/RESET#)
      (node (ref U3) (pin 29))
      (node (ref P22) (pin 3)))
    (net (code 96) (name /hackrf_if/H1_CPLD_TCK)
      (node (ref P28) (pin 17))
      (node (ref U3) (pin 16)))
    (net (code 97) (name /hackrf_if/PP_CPLD_TMS)
      (node (ref P28) (pin 8))
      (node (ref U3) (pin 14)))
    (net (code 98) (name "Net-(P28-Pad16)")
      (node (ref P28) (pin 16)))
    (net (code 99) (name /hackrf_if/MCU_LCD_RD)
      (node (ref P22) (pin 5))
      (node (ref U3) (pin 30)))
    (net (code 100) (name "Net-(U3-Pad35)")
      (node (ref U3) (pin 35)))
    (net (code 101) (name "Net-(U3-Pad36)")
      (node (ref U3) (pin 36)))
    (net (code 102) (name "Net-(U3-Pad7)")
      (node (ref U3) (pin 7)))
    (net (code 103) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 104) (name /hackrf_if/MCU_DIR)
      (node (ref U3) (pin 42))
      (node (ref P22) (pin 22)))
    (net (code 105) (name /hackrf_if/P2_8)
      (node (ref U3) (pin 34))
      (node (ref P22) (pin 23)))
    (net (code 106) (name /hackrf_if/MCU_ADDR)
      (node (ref U3) (pin 33))
      (node (ref P22) (pin 19)))
    (net (code 107) (name /hackrf_if/MCU_LCD_WR)
      (node (ref P22) (pin 21))
      (node (ref U3) (pin 40)))
    (net (code 108) (name /hackrf_if/MCU_IO_STBX)
      (node (ref P22) (pin 20))
      (node (ref U3) (pin 32)))
    (net (code 109) (name "Net-(P22-Pad2)")
      (node (ref P22) (pin 2)))
    (net (code 110) (name /hackrf_if/MCU_LCD_TE)
      (node (ref P22) (pin 6))
      (node (ref U3) (pin 31)))
    (net (code 111) (name "Net-(J3-Pad33)")
      (node (ref J3) (pin 33)))
    (net (code 112) (name /lcd_sw_sd/LEDK2)
      (node (ref J3) (pin 3))
      (node (ref U4) (pin 4)))
    (net (code 113) (name /lcd_sw_sd/LEDK1)
      (node (ref J3) (pin 2))
      (node (ref U4) (pin 3)))
    (net (code 114) (name /lcd_sw_sd/LEDK3)
      (node (ref J3) (pin 4))
      (node (ref U4) (pin 5)))
    (net (code 115) (name /lcd_sw_sd/LEDK4)
      (node (ref U4) (pin 6))
      (node (ref J3) (pin 5)))
    (net (code 116) (name "Net-(R20-Pad1)")
      (node (ref R20) (pin 1))
      (node (ref U4) (pin 7)))
    (net (code 117) (name "Net-(R6-Pad1)")
      (node (ref U6) (pin 16))
      (node (ref R6) (pin 1)))
    (net (code 118) (name "Net-(R4-Pad1)")
      (node (ref U6) (pin 12))
      (node (ref R4) (pin 1)))
    (net (code 119) (name "Net-(R1-Pad1)")
      (node (ref U6) (pin 14))
      (node (ref R1) (pin 1)))
    (net (code 120) (name "Net-(R8-Pad1)")
      (node (ref R8) (pin 1))
      (node (ref U6) (pin 1)))
    (net (code 121) (name "Net-(R10-Pad1)")
      (node (ref R10) (pin 1))
      (node (ref U6) (pin 15)))
    (net (code 122) (name "Net-(R13-Pad2)")
      (node (ref R13) (pin 2))
      (node (ref U6) (pin 6)))
    (net (code 123) (name "Net-(R14-Pad1)")
      (node (ref R14) (pin 1))
      (node (ref U6) (pin 5)))
    (net (code 124) (name "Net-(D1-PadA)")
      (node (ref R3) (pin 2))
      (node (ref D1) (pin A)))
    (net (code 125) (name "Net-(D1-PadC)")
      (node (ref D1) (pin C))
      (node (ref U6) (pin 7)))
    (net (code 126) (name "Net-(D2-PadA)")
      (node (ref D2) (pin A))
      (node (ref R5) (pin 2)))
    (net (code 127) (name "Net-(D2-PadC)")
      (node (ref U6) (pin 9))
      (node (ref D2) (pin C)))
    (net (code 128) (name /power/BBAT)
      (node (ref C15) (pin 1))
      (node (ref U6) (pin 2))
      (node (ref U6) (pin 3))
      (node (ref J4) (pin 1)))
    (net (code 129) (name "Net-(R9-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref U6) (pin 4)))
    (net (code 130) (name "Net-(C39-Pad1)")
      (node (ref C39) (pin 1))
      (node (ref U2) (pin 4)))
    (net (code 131) (name /hackrf_if/LCD_DB13)
      (node (ref J3) (pin 19))
      (node (ref U3) (pin 45)))
    (net (code 132) (name /hackrf_if/LCD_DB2)
      (node (ref U3) (pin 56))
      (node (ref J3) (pin 30)))
    (net (code 133) (name /hackrf_if/LCD_DB3)
      (node (ref U3) (pin 55))
      (node (ref J3) (pin 29)))
    (net (code 134) (name /hackrf_if/LCD_DB4)
      (node (ref U3) (pin 54))
      (node (ref J3) (pin 28)))
    (net (code 135) (name /hackrf_if/LCD_DB5)
      (node (ref U3) (pin 53))
      (node (ref J3) (pin 27)))
    (net (code 136) (name /hackrf_if/LCD_DB6)
      (node (ref J3) (pin 26))
      (node (ref U3) (pin 52)))
    (net (code 137) (name /hackrf_if/LCD_DB7)
      (node (ref J3) (pin 25))
      (node (ref U3) (pin 51)))
    (net (code 138) (name /hackrf_if/LCD_DB8)
      (node (ref U3) (pin 50))
      (node (ref J3) (pin 24)))
    (net (code 139) (name /hackrf_if/LCD_DB9)
      (node (ref J3) (pin 23))
      (node (ref U3) (pin 49)))
    (net (code 140) (name /hackrf_if/LCD_DB10)
      (node (ref J3) (pin 22))
      (node (ref U3) (pin 48)))
    (net (code 141) (name /hackrf_if/LCD_DB11)
      (node (ref U3) (pin 47))
      (node (ref J3) (pin 21)))
    (net (code 142) (name /hackrf_if/LCD_DB12)
      (node (ref U3) (pin 46))
      (node (ref J3) (pin 20)))
    (net (code 143) (name /hackrf_if/LCD_DB14)
      (node (ref U3) (pin 44))
      (node (ref J3) (pin 18)))
    (net (code 144) (name /hackrf_if/LCD_DB15)
      (node (ref J3) (pin 17))
      (node (ref U3) (pin 43)))
    (net (code 145) (name /hackrf_if/LCD_DB0)
      (node (ref U3) (pin 59))
      (node (ref J3) (pin 32)))
    (net (code 146) (name /hackrf_if/LCD_DB1)
      (node (ref U3) (pin 58))
      (node (ref J3) (pin 31)))))